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There is only one adjustment, assuming that you have built the circuit as described, and that
is to adjust P1 so that the Drain pin of Q1 is set at 10 volts DC. After you have set P1, you
need to let the amplifier spend some time warming up, say a half hour, and then adjust it to 10
volts again. Then do this one last time after another half hour.

While the amplifier is warming up, the cover should be set in place so as to simulate the
ventilation that the channel will experience under the same thermal conditions as normal
operation.

That all there is to it.




