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Adopting the cone type of the 30cm aperture where in the limits the carbon fiber is mixed low in the cone paper.
In addition, the copper cap being attached magnetic circuit which phenomenon it can point the electric current strain is used.

The unit which designates the hard duralmin dome of the 4.8cm aperture as the diaphragm is adopted to the middle limits. Quality is arranged on the diaphragm front, the diffuser of precise die-cast directivity is improved simultaneously has been attached. In order to lose the masking effect of sound, it is the design which provides the multiple hole.

To the eater has adopted the hard titanium dome diaphragm of the 2.5cm aperture. The stainless steel wool is used to the braking material.
In addition, mid range similar and the radial diffuser of precise die-cast make are loaded, directivity is improved.

To mid range floating mount system is adopted for fixing of the eater, IM distortion occurrence because of this with the influence from the woofer is held down, is designed in such a way that unit original quality is not impaired. In addition, the baffle plate and the liner take complete installed structure together, have become the strong making.

The empty core coil metallurgy being attached tunic condenser of 1.2mm is adopted to network. In addition, non induction winding high resistance input [atsuteneta] of new development is adopted to [atsuteneta] for mediant.

　

	Rating of type

	System
	3 ways 3 speakers airtightness system bookshelf type

	Use unit
	It is low the for limits: 30cm cone type
For middle limits: 4.8cm dome type
For high pass: 2.5cm dome type

	Impedance
	8Ω

	Playback frequency zone
	35Hz~20000Hz

	Output overpressure value
	91.5dB/W/m

	Largest input
	80W

	Crossover frequency
	1000Hz and 5200Hz

	External size
	Width 380× height 660× depth 317mm

	Weight
	21kg


