	LS-26 assembled & tested

	US$102.00
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circuit modify from convergent SL-1,have two voltage amplify stage, 12AU7 used in first stage,second stage is 12AX7 SRPP, output stage use a  6DJ8 as a cathode follower,voltage swing about 50V.With more dynamic ,mid and high end is lush, liquid and detail.  PP coupling capacitor,metal film and carbon film resistor, tubes are used but test good most are US made

(case and power transformer not included)
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